Guidelines

These guidelines are for entrances on county maintained roads only. Entrances on township roads are governed by the township boards.

**NEW ENTRANCES**

New approved entrance culverts will be purchased by the landowner from Wabaunsee County and installed by county crews. They will be rocked and maintained to the right-of-way. Entrances then become the property of Wabaunsee County.

**EXISTING ENTRANCES**

Existing entrances that are to be upgraded will be charged to the landowner. Charges will include culvert pipe, cover materials, labor and equipment. An estimate for these charges will precede actual installation.

**(Please keep in mind several factors when marking your location)**

1. Have at least 350’ of sight distance in both directions.
2. Make sure brush is not within the sight line.
3. The larger the drainage area upstream, the larger the diameter of pipe will be needed, therefore increasing your cost.
4. Driveways (including circle) must have a minimum of 185’ of space between entrances and depending on the road classification may require 300’ to 350’ spacing.
5. The entrance needs to be 200’ to 300’ from intersection depending on the roadway classification.